          
     To install, copy the file SCO.DRV to a formatted floppy:
          
     dd if=sco.drv of=/dev/fd0135ds18
          
     Then invoke 'custome'.
          
     The filename from metabyte is called xsco9680.drv. If the above 
     procedure does not work, try to change name.
     
