This file is best viewed with word wrap turned on.

1.  To install or upgrade the STB Velocity 4400 device driver, double-click the Setup and follow the on-screen instructions.

2.  If you want to make installation diskettes, copy only the files from within each directory (disk1 to disk4) onto each of four diskettes. Then run Setup from the first diskette.

3.  If this is a new installation, you will have the option of installing the enclosed STB Velocity 4400 graphics device driver.

4.  If you have a previous STB Velocity 4400 device driver, and have obtained an updated STB Velocity 4400 device driver - this installation will give you the option of upgrading your current driver to the one enclosed.

5.  If Vision '98 is currently resident or installed on your system, this driver upgrade will remove it.  Vision '98 will no longer be available after the driver upgrade has been installed.  Vision '98 Monitor Properties and independent Desktop Area and Resolution settings will no longer be available once Vision '98 is removed.

Note:  Please refer to the Settings Tab in the Display Properties Page to adjust screen resolutions and refresh rates.  This driver upgrade will improve the performance and stability of your Velocity 4400 Display Adapter.

